| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
_sctp_tmp_info Struct Reference

Transient per-packet info collected during SCTP dissection before a full association record exists. More...

`#include <tap-sctp-analysis.h>`

## Public Attributes
uint16_t | assoc_id
uint16_t | direction
address | src
address | dst
uint16_t | port1
uint16_t | port2
uint32_t | verification_tag1
uint32_t | verification_tag2
uint32_t | initiate_tag
uint32_t | n_tvbs

## Detailed Description

Transient per-packet info collected during SCTP dissection before a full association record exists.

## Member Data Documentation

## ◆ assoc_id

uint16_t _sctp_tmp_info::assoc_id

Temporary association identifier assigned during dissection.

## ◆ direction

uint16_t _sctp_tmp_info::direction

Packet direction relative to the association endpoints.

## ◆ dst

address _sctp_tmp_info::dst

Destination address of the SCTP packet.

## ◆ initiate_tag

uint32_t _sctp_tmp_info::initiate_tag

Initiate tag extracted from the INIT or INIT-ACK chunk.

## ◆ n_tvbs

uint32_t _sctp_tmp_info::n_tvbs

Number of tvbuffs referenced by this packet.

## ◆ port1

uint16_t _sctp_tmp_info::port1

Source port number.

## ◆ port2

uint16_t _sctp_tmp_info::port2

Destination port number.

## ◆ src

address _sctp_tmp_info::src

Source address of the SCTP packet.

## ◆ verification_tag1

uint32_t _sctp_tmp_info::verification_tag1

Verification tag for endpoint 1.

## ◆ verification_tag2

uint32_t _sctp_tmp_info::verification_tag2

Verification tag for endpoint 2.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/ui/tap-sctp-analysis.h