| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
tagApduStatusSwitch Struct Reference

Carries the link-layer addressing context needed to correlate APDU status frames in a redundant PROFINET topology. More...

`#include <packet-pn.h>`

## Public Attributes
bool | isRedundancyActive
address | dl_dst
address | dl_src

## Detailed Description

Carries the link-layer addressing context needed to correlate APDU status frames in a redundant PROFINET topology.

## Member Data Documentation

## ◆ dl_dst

address tagApduStatusSwitch::dl_dst

Data-link destination address of the APDU status frame.

## ◆ dl_src

address tagApduStatusSwitch::dl_src

Data-link source address of the APDU status frame.

## ◆ isRedundancyActive

bool tagApduStatusSwitch::isRedundancyActive

True if PROFINET system redundancy is currently active for this station.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/plugins/epan/profinet/packet-pn.h