| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
blf_linmessage Struct Reference

Header for a BLF LIN message object (legacy format) carrying up to 8 data bytes. More...

`#include <blf.h>`

## Public Attributes
uint16_t | channel
uint8_t | id
uint8_t | dlc
uint8_t | data [8]
uint8_t | fsmId
uint8_t | fsmState
uint8_t | headerTime
uint8_t | fullTime
uint16_t | crc
uint8_t | dir
uint8_t | res1

## Detailed Description

Header for a BLF LIN message object (legacy format) carrying up to 8 data bytes.

## Member Data Documentation

## ◆ channel

uint16_t blf_linmessage::channel

Logical LIN channel number on which this message was captured.

## ◆ crc

uint16_t blf_linmessage::crc

Checksum of the LIN frame (classic or enhanced).

## ◆ data

uint8_t blf_linmessage::data[8]

Payload data bytes of the LIN frame.

## ◆ dir

uint8_t blf_linmessage::dir

Transfer direction: 0 = RX, 1 = TX Receipt, 2 = TX Request.

## ◆ dlc

uint8_t blf_linmessage::dlc

Data Length Code indicating the number of data bytes (0–8).

## ◆ fsmId

uint8_t blf_linmessage::fsmId

Identifier of the finite state machine instance that processed this frame.

## ◆ fsmState

uint8_t blf_linmessage::fsmState

State of the finite state machine at the time this frame was processed.

## ◆ fullTime

uint8_t blf_linmessage::fullTime

Total duration of the complete LIN frame in bit times.

## ◆ headerTime

uint8_t blf_linmessage::headerTime

Duration of the LIN header in bit times.

## ◆ id

uint8_t blf_linmessage::id

LIN frame identifier (0–63).

## ◆ res1

uint8_t blf_linmessage::res1

Reserved; must be zero.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/wiretap/blf.h