| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
dis_tap_info Struct Reference

## Public Attributes
bool | info_valid_radio_pdu_tap
uint8_t | info_pdu_type
uint16_t | info_radio_id
uint16_t | info_entity_id_site
uint16_t | info_entity_id_appl
uint16_t | info_entity_id_entity
uint8_t | info_transmit_state
uint8_t | info_radio_input_source
uint8_t | info_payload_type
uint32_t | info_tx_timestamp
uint32_t | info_sample_rate
uint32_t | info_num_samples
bool | info_all_data_present
unsigned | info_payload_offset
unsigned | info_payload_len
const uint8_t * | info_data
const char * | info_payload_type_str

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/epan/dissectors/packet-dis.h