| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
_e_guid_t Struct Reference

Represents a GUID/UUID value; may be larger than GUID_LEN so must not be used to directly overlay packet data. More...

`#include <guid-utils.h>`

## Public Attributes
uint32_t | data1
uint16_t | data2
uint16_t | data3
uint8_t | data4 [8]

## Detailed Description

Represents a GUID/UUID value; may be larger than GUID_LEN so must not be used to directly overlay packet data.

## Member Data Documentation

## ◆ data1

uint32_t _e_guid_t::data1

First component of the GUID: the 32-bit time-low field.

## ◆ data2

uint16_t _e_guid_t::data2

Second component of the GUID: the 16-bit time-mid field.

## ◆ data3

uint16_t _e_guid_t::data3

Third component of the GUID: the 16-bit time-high-and-version field.

## ◆ data4

uint8_t _e_guid_t::data4[8]

Fourth component of the GUID: the 8-byte clock sequence and node fields.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/epan/guid-utils.h