| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Here is a list of all documented variables with links to the class documentation for each member:

### - c -

- c2s : _RRPD
- calculation : _RRPD
- call : _extcap_arg, _extcap_interface, _extcap_value
- call_active_state : _voip_calls_info, _voip_packet_info_t
- call_comment : _voip_calls_info, _voip_packet_info_t
- call_id : _voip_calls_info, _voip_packet_info_t
- call_identifier : _sip_calls_info
- call_num : _rtpstream_info, _voip_calls_info, ascend_phdr
- call_state : _unistim_info_t, _voip_calls_info, _voip_packet_info_t
- callback : _ext_menubar_t, _ext_toolbar_t, _funnel_packet_menu_t
- callback_data : _funnel_packet_menu_t
- callbacks : _wmem_allocator_t
- callId : _skinny_calls_info
- callsinfo_hashtable : _voip_calls_tapinfo
- callsinfos : _voip_calls_tapinfo
- can_check_fcs : ws80211_interface
- can_desegment : _packet_info
- can_expand : wslua_variable_t
- can_set_freq : ws80211_interface
- can_set_rfmon : if_capabilities_t
- can_tls : tcpcl_peer_t
- can_write_encap : file_type_subtype_info
- can_write_encap_ref : _wslua_filehandler
- cancel_acks : ltp_session_data_t
- cancels : ltp_session_data_t
- canExpand : LuaDebuggerPath::VariableRowFields
- canfdflags : blf_canfdmessage
- cap_end_time : _summary_tally
- cap_file_ : MainStatusBar, PrintDialog, WiresharkDialog
- cap_len : _frame_data
- cap_monitor : ws80211_interface
- cap_pipe_bytes_read : _capture_src
- cap_pipe_bytes_to_read : _capture_src
- cap_pipe_databuf : _capture_src
- cap_pipe_databuf_size : _capture_src
- cap_pipe_fd : _capture_src
- cap_pipe_max_pkt_size : _capture_src
- cap_pipe_modified : _capture_src
- cap_start_time : _summary_tally
- capfile : WirelessTimeline
- caplen : ascend_state_t, wtap_packet_header
- caps : if_info_t
- caption_ : EditorFileDialog
- capture : _extcap_parameters
- capture_auto_scroll : recent_settings_tag
- capture_child : capture_options_tag
- capture_device : _e_prefs
- capture_devices_buffersize : _e_prefs
- capture_devices_descr : _e_prefs
- capture_devices_filter : _e_prefs
- capture_devices_hide : _e_prefs
- capture_devices_linktypes : _e_prefs
- capture_devices_monitor_mode : _e_prefs
- capture_devices_pmode : _e_prefs
- capture_devices_snaplen : _e_prefs
- capture_file_ : MainWindow
- capture_filter : _extcap_parameters
- capture_filters_list : capture_options_tag
- capture_gentime : erf_private
- capture_icon_ : MainApplication
- capture_monitor_mode : _e_prefs
- capture_no_extcap : _e_prefs
- capture_no_interface_load : _e_prefs
- capture_only : _ext_toolbar_t
- capture_pcap_ng : _e_prefs
- capture_position : _TSUM_PREFERENCES
- capture_prom_mode : _e_prefs
- capture_real_time : _e_prefs
- capture_show_info : _e_prefs
- capture_update_interval : _e_prefs
- captured_size : packet_entry_header
- cb : _uat_field_t
- cb_func : _tap_reg, _wtap_module_reg
- cb_name : _tap_reg, _wtap_module_reg
- cbData : AmsHead
- cbdata : _uat_field_t
- cbLength : AdsNotificationAttrib, TAdsDeviceNotificationReq, TAdsReadReq, TAdsReadRes, TAdsReadWriteRes
- Ccs : tSdoHeaderUnion
- ceil : _range_pair
- cells : atm_phdr
- cf : match_data, packet_range_tag
- cf_count : _ws_info_t
- cf_filename : _ws_info_t
- cf_framenr : _ws_info_t
- cf_state : _ws_info_t
- cfg : _mate_gog, _mate_gop, _mate_pdu, _stats_tree
- cfilter : iface_summary_info_tag, interface_options_tag, interface_tag
- change_value : decode_as_s
- changed : epan_uat
- changed_in_pkn : quic_pp_state
- changes : _bluetooth_device_tapinfo_t, _bluetooth_item_data_t
- Channel : tMbxHeaderControlUnion
- channel : atm_phdr, blf_canerror, blf_canerrorext, blf_canfderror64, blf_canfdmessage64, blf_canfdmessage, blf_canmessage, blf_canxlchannelframe, blf_ethernet_phystate, blf_ethernet_rxerror, blf_ethernet_status, blf_ethernetframeheader, blf_ethernetframeheader_ex, blf_flexraydata, blf_flexraymessage, blf_flexrayrcvmessage, blf_flexrayrcvmessageex, blf_linbusevent, blf_linmessage, blf_linrcverror, blf_linsenderror, blf_linsleepmodeevent, blf_linwakeupevent, blf_wlanframeheader, bthci_phdr, gsm_um_phdr, ieee_802_11_phdr, isdn_phdr
- channel_handles : ssh_peer_data
- channel_info : ssh_peer_data
- channel_mask : ws80211_frequency
- channel_type : ieee_802_11a
- channel_types : ws80211_band
- channelId : rlc_graph, rlc_segment
- channelMask : blf_flexrayrcvmessage, blf_flexrayrcvmessageex
- channels : _codec_context_t
- channelSet : rlc_graph
- channelType : rlc_graph, rlc_segment
- chdr_missing : tcpcl_peer_t
- chdr_seen : tcpcl_peer_t
- check_address : _sctp_assoc_info
- checkpoints : ltp_session_data_t
- checksum_type : _sctp_assoc_info
- checksumModel : blf_linmessagedescriptor
- child : _phs_t
- childItems_ : ModelHelperTreeItem< Item >
- childPath : LuaDebuggerPath::VariableRowFields
- children : _ext_menubar_t, _ext_toolbar_t, _oid_info_t, _sctp_allassocs_info, _stat_node, pbl_node_t
- children_by_name : pbl_node_t
- chk : _uat_field_t
- chkp_acks : ltp_session_data_t
- chunk : ascend_phdr
- chunk_count : _sctp_assoc_info
- chunk_info : _sctp_error_info
- chunktype : mmodule_phdr
- cic : _isup_calls_info
- cid : k12_input_info_t
- cidr_addr : hashipv4, hashipv6
- cinfo : _packet_info, _wslua_col_info, _wslua_cols
- cipher : _DOT11DECRYPT_ASSOC_PARSED, _DOT11DECRYPT_EAPOL_PARSED, _DOT11DECRYPT_SEC_ASSOCIATION, SslPacketInfo
- cipher_algo : quic_info_data
- cipher_mode : quic_info_data
- city : _mmdb_lookup_t
- class_meta : _wslua_class
- class_methods : _wslua_class
- class_name : ias_class_dissector
- cleanup : _stats_tree_cfg, _wmem_allocator_t, dfilter_plugin, epan_plugin
- cleanup_postkill_cb : _extcap_parameters
- clear : _GRealArray
- clear_func : _GRealArray
- clear_text : _funnel_ops_t
- clflags_offset : nstr_phdr
- cli_string : _stat_tap_table_ui, _stat_tap_ui
- client_cids : quic_info_data
- client_dcid_initial : quic_info_data
- client_dcid_set : quic_info_data
- client_grease_quic_bit : quic_info_data
- client_index : blf_logobjectheader
- client_ip : _follow_info
- client_iv : ua_keyset
- client_key : ua_keyset
- client_key_len : ua_keyset
- client_loss_bits_recv : quic_info_data
- client_loss_bits_send : quic_info_data
- client_multipath : quic_info_data
- client_odcid : quic_info_data
- client_port : _follow_info
- client_retry_processed : quic_info_data
- client_sig_len : ua_keyset
- client_streams : quic_info_data
- clientIndex : blf_flexrayrcvmessage, blf_flexrayrcvmessageex
- clientIndexFlexRayV6Message : blf_flexraymessage
- clnp_dstref : _packet_info
- clnp_srcref : _packet_info
- clock_drift_ms : _rtpstream_info_calc
- clock_rate : _tap_rtp_stat_t
- clockMode : blf_ethernet_status
- close_cb_data : _wslua_tw
- close_dialogs : _funnel_ops_t
- closed_msg : capture_options_tag
- clusterNo : blf_flexrayrcvmessage, blf_flexrayrcvmessageex
- clusterTime : blf_flexraymessage
- Cmd : TEFWUPDATE_HEADER
- cmd : _EcParser, gryphon_pkt_info_t, print_args_t
- cmd_context : gryphon_pkt_info_t
- cmdId : AmsHead
- code : _rose_ctx_t, df_error_t, nghttp2_huff_sym, wtap_bpf_insn_s
- code_global : _rose_ctx_t
- code_item : _rose_ctx_t
- code_local : _rose_ctx_t
- coding_known : ieee_802_11be_user_info
- col : _wslua_col_info
- col_buf : col_item_t
- col_custom_dfilter : col_item_t
- col_custom_fields : col_item_t
- col_custom_fields_ids : col_item_t
- col_custom_occurrence : col_item_t
- col_data : col_item_t
- col_expr : col_expr_t, epan_column_info
- col_expr_val : col_expr_t
- col_fence : col_item_t
- col_first : epan_column_info
- col_fmt : col_item_t, epan_app_data_t
- col_last : epan_column_info
- col_len : _dfilter_loc
- col_list : _e_prefs
- col_start : _dfilter_loc
- col_title : col_item_t
- col_width_list : recent_settings_tag
- colDuration : timeline_span
- colnum : _fld_data_t
- color : _io_graph_settings_t, _plot_settings_t, _wmem_tree_node_t, HexDataSourceView::ByteViewAnnotation
- color_ : Graph
- color_edt : file_data_s, frame_data_s
- color_end : SlideTypeConfig
- color_filter : _frame_data
- color_gradient : SlideTypeConfig
- color_start : SlideTypeConfig
- ColoringRulesMimeType : WiresharkMimeData
- cols_hide_new : _e_prefs
- colStart : timeline_span
- column_name : _stat_tap_table_item
- ColumnListMimeType : WiresharkMimeData
- columns : epan_column_info
- columns_ : ProfileModel
- comId : ComId
- command_line : procmon_process_t
- comment : _seq_analysis_item, filter_expression, HexDataSourceView::ByteViewAnnotation
- comp_gencnt : darwin_md
- company : procmon_module_t, procmon_process_t
- compare : _ftype_t
- compat : _c_encoded
- compiled_with : _extcap_parameters
- Complete : tSdoHeaderUnion
- completed : thread_pool
- completed_calls : _voip_calls_tapinfo
- completer_ : SyntaxLineEdit
- completion_model_ : SyntaxLineEdit
- complex_type : _extcap_complex
- compress_type : capture_options_tag
- compression_level : blf_fileheader
- compression_method : blf_logcontainerheader
- compression_type : _summary_tally, wtap_dumper
- compute_option_size : compute_options_size_t
- condition : _tvbparse_wanted_t, _wslua_breakpoint_t
- condition_error : _wslua_breakpoint_t
- condition_error_msg : _wslua_breakpoint_t
- conditions : tlv_wireless_info
- config_error : _mate_config
- config_option_name : _extcap_parameters
- config_option_value : _extcap_parameters
- config_stack : _mate_config
- configurable : _extcap_arg
- configuredNodeAddress : blf_linmessagedescriptor
- conn_addr : media_description_t, session_info_t
- connector : blf_ethernet_status
- consconns : cba_ldev_s
- consframes : cba_ldev_s
- console_name : commandline_usage_app_data
- contact_negotiated : tcpcl_conversation_t
- contained_length : tvbuff
- contains : _ftype_t
- content_id : media_content_info_t
- content_len : _SslRecordInfo
- content_type : _export_object_entry_t
- context : _dof_secmode_api_data
- context_id : bpsec_id_t
- contiguous_len : _fragment_head
- Control : tMbxHeaderControlUnion, tSdoControlUnion, tSoeHeaderControlUnion
- control : _extcap_info, _extcap_interface, _tvbparse_wanted_t
- control_in : _extcap_parameters
- control_in_fd : _extcap_parameters
- control_out : _extcap_parameters
- control_out_fd : _extcap_parameters
- control_out_queue : interface_values
- control_port : media_description_t
- control_uri : media_description_t
- controls : _iface_toolbar
- conv : _wslua_conv_data_t, edhoc_state_t
- conv_addr_port_endpoints : _packet_info
- conv_array : _conversation_hash_t
- conv_elements : _packet_info
- conv_id : _conversation_item_t, _conversation_key_t
- conv_index : conversation
- conv_machine_readable : _e_prefs
- conv_num : _seq_analysis_item
- conversation_deinterlacing_key : _e_prefs
- conversation_tabs : recent_settings_tag
- conversation_tabs_columns : recent_settings_tag
- conversation_type_val : conversation_element
- copy_allowed : wtap_custom_block_header
- copy_bt_ : TrafficTableDialog
- copy_cb : epan_uat
- copy_mand : wtap_blocktype_t
- copy_to_clipboard : _funnel_ops_t
- copy_value : _ftype_t
- copyright : mpa
- coreid_offset : nstr_phdr
- corr_orig : ltp_tap_info_t
- cosine : wtap_pseudo_header
- count : _burst_bucket, _tap_rtp_save_info_t, buffer, i4b_trace_hdr_t, next_tvb_list_t, thread_pool
- Counter : tMbxHeaderControlUnion
- counter : _stat_node
- CountNV : _NvParserHDR
- country : _mmdb_lookup_t
- country_iso : _mmdb_lookup_t
- counts : _capture_info, _capture_packet_info, _info_data
- cpu1 : pcaprec_ss990915_hdr
- cpu2 : pcaprec_ss990915_hdr
- cpu_id : wtap_syscall_header
- crc : blf_canfderror64, blf_canfdmessage64, blf_canxlchannelframe, blf_flexraydata, blf_lincrcerror2, blf_linmessage2, blf_linmessage
- crc_field : bp_block_canonical_t, bp_block_primary_t
- crc_type : bp_block_canonical_t, bp_block_primary_t
- create : wtap_blocktype_t
- created : _wslua_distbl_t
- created_item : _asn1_ctx_t
- criterium : _mate_cfg_pdu
- criterium_accept_mode : _mate_cfg_pdu
- criterium_match_mode : _mate_cfg_pdu
- crumb_bit_length : crumb_spec_t
- crumb_bit_offset : crumb_spec_t
- crv : _actrace_isdn_calls_info
- crypto_offset : _quic_crypto_info
- CS : tSdoHeaderUnion
- cs_count_ : MainStatusBar
- cs_fixed_ : MainStatusBar
- ctime : _fileset_entry
- ctrl_role : _iface_toolbar_control
- ctrl_type : _iface_toolbar_control
- ctx_ : GLibPoller
- ctype : _conversation_item_t
- cum_bytes : _frame_data
- cum_tsn_ack : nr_sack_chunk_header, sack_chunk_header
- cur_layout_ : MainWindow
- cur_loc : tcpcl_dissect_ctx_t
- curr_layer_num : _packet_info, _packet_proto_data_t
- curr_proto_layer_num : _packet_info
- current : _fileset_entry
- current_center_freq1 : ws80211_iface_info
- current_center_freq2 : ws80211_iface_info
- current_chan_type : ws80211_iface_info
- current_depth : json_dumper
- current_fcs_validation : ws80211_iface_info
- current_frame : packet_range_iter
- current_freq : ws80211_iface_info
- current_items : _mate_runtime_data
- current_namespace : ieee80211_radiotap_iterator
- current_proto : _packet_info
- current_section_number : pcapng_t
- current_stream : _http3_session_info
- currentFile : TrdpXmlContext
- custom_binaryval : wtap_optval_t
- custom_block_data : section_info_t
- custom_block_header : wtap_rec
- custom_cbs : preference
- custom_colors : recent_settings_tag
- custom_data : binary_optdata
- custom_data_len : binary_optdata
- custom_fields : _fmt_data
- custom_occurrence : _fmt_data
- custom_stringval : wtap_optval_t
- cycle : blf_flexraymessage, blf_flexrayrcvmessage, blf_flexrayrcvmessageex
- CycleIndex : _NvParserHDR
- cycles : _tap_iax2_stat_t