| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
_h323_calls_info Struct Reference

Protocol-specific call metadata for H.323 calls. More...

`#include <voip_calls.h>`

## Public Attributes
e_guid_t * | guid
GList * | h245_list
address | h225SetupAddr
bool | is_h245
bool | is_faststart_Setup
bool | is_faststart_Proc
bool | is_h245Tunneling
int32_t | q931_crv
int32_t | q931_crv2
unsigned | requestSeqNum

## Detailed Description

Protocol-specific call metadata for H.323 calls.

## Member Data Documentation

## ◆ guid

e_guid_t* _h323_calls_info::guid

H.225 Call ID GUID uniquely identifying this H.323 call.

## ◆ h225SetupAddr

address _h323_calls_info::h225SetupAddr

Source IP from the H.225 SETUP message, used to determine packet direction.

## ◆ h245_list

GList* _h323_calls_info::h245_list

List of h245_address_t entries for tunnelled H.245 channels.

## ◆ is_faststart_Proc

bool _h323_calls_info::is_faststart_Proc

True if a fastStart element was present in Proceeding, Alerting, Progress, or Connect.

## ◆ is_faststart_Setup

bool _h323_calls_info::is_faststart_Setup

True if a fastStart element was present in the H.225 SETUP message.

## ◆ is_h245

bool _h323_calls_info::is_h245

True if a separate H.245 control channel has been detected.

## ◆ is_h245Tunneling

bool _h323_calls_info::is_h245Tunneling

True if H.245 messages are tunnelled inside H.225 messages.

## ◆ q931_crv

int32_t _h323_calls_info::q931_crv

Q.931 Call Reference Value for the forward direction.

## ◆ q931_crv2

int32_t _h323_calls_info::q931_crv2

Q.931 Call Reference Value for the reverse direction.

## ◆ requestSeqNum

unsigned _h323_calls_info::requestSeqNum

H.225 RAS request sequence number for matching responses.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/ui/voip_calls.h