| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
ieee_802_11ax Struct Reference

PHY metadata for 802.11ax (HE — High Efficiency) captures. More...

`#include <wtap.h>`

## Public Attributes
unsigned | has_mcs_index: 1
unsigned | has_bwru: 1
unsigned | has_gi: 1
uint8_t | nsts: 4
uint8_t | mcs: 4
uint8_t | bwru: 4
uint8_t | gi: 2

## Detailed Description

PHY metadata for 802.11ax (HE — High Efficiency) captures.

## Member Data Documentation

## ◆ bwru

uint8_t ieee_802_11ax::bwru

Bandwidth or Resource Unit (RU) allocation identifier.

## ◆ gi

uint8_t ieee_802_11ax::gi

Guard interval: encodes 0.8 µs, 1.6 µs, or 3.2 µs GI.

## ◆ has_bwru

unsigned ieee_802_11ax::has_bwru

Non-zero if `bwru` contains a valid value.

## ◆ has_gi

unsigned ieee_802_11ax::has_gi

Non-zero if `gi` contains a valid value.

## ◆ has_mcs_index

unsigned ieee_802_11ax::has_mcs_index

Non-zero if `mcs` contains a valid value.

## ◆ mcs

uint8_t ieee_802_11ax::mcs

Modulation and Coding Scheme (MCS) index for this HE transmission.

## ◆ nsts

uint8_t ieee_802_11ax::nsts

Number of Space-Time Streams used for this HE transmission.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/wiretap/wtap.h