| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
blf_ethernetframeheader Struct Reference

Header for a BLF Ethernet frame object (legacy format). More...

`#include <blf.h>`

## Public Attributes
uint8_t | src_addr [6]
uint16_t | channel
uint8_t | dst_addr [6]
uint16_t | direction
uint16_t | ethtype
uint16_t | tpid
uint16_t | tci
uint16_t | payloadlength
uint64_t | res

## Detailed Description

Header for a BLF Ethernet frame object (legacy format).

## Member Data Documentation

## ◆ channel

uint16_t blf_ethernetframeheader::channel

Logical channel number on which this frame was captured.

## ◆ direction

uint16_t blf_ethernetframeheader::direction

Transfer direction: one of BLF_DIR_RX, BLF_DIR_TX, or BLF_DIR_TX_RQ.

## ◆ dst_addr

uint8_t blf_ethernetframeheader::dst_addr[6]

Destination MAC address of the Ethernet frame.

## ◆ ethtype

uint16_t blf_ethernetframeheader::ethtype

EtherType field identifying the encapsulated protocol.

## ◆ payloadlength

uint16_t blf_ethernetframeheader::payloadlength

Length in bytes of the Ethernet payload.

## ◆ res

uint64_t blf_ethernetframeheader::res

Reserved; must be zero.

## ◆ src_addr

uint8_t blf_ethernetframeheader::src_addr[6]

Source MAC address of the Ethernet frame.

## ◆ tci

uint16_t blf_ethernetframeheader::tci

Tag Control Information for VLAN-tagged frames (PCP, DEI, VID).

## ◆ tpid

uint16_t blf_ethernetframeheader::tpid

Tag Protocol Identifier for VLAN-tagged frames (802.1Q TPID).

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/wiretap/blf.h