| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
rtp_frame_info Struct Reference

Structure used for storing frame num during visual waveform decoding. More...

`#include <rtp_audio_file.h>`

## Public Attributes
qint64 | real_pos
qint64 | sample_pos
qint64 | len
uint32_t | frame_num
rtp_frame_type | type

## Detailed Description

Structure used for storing frame num during visual waveform decoding.

## Member Data Documentation

## ◆ frame_num

uint32_t rtp_frame_info::frame_num

The RTP frame number.

## ◆ len

qint64 rtp_frame_info::len

The length of the frame data.

## ◆ real_pos

qint64 rtp_frame_info::real_pos

The real position in the byte stream.

## ◆ sample_pos

qint64 rtp_frame_info::sample_pos

The logical sample position.

## ◆ type

rtp_frame_type rtp_frame_info::type

The type of the RTP frame.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/ui/qt/utils/rtp_audio_file.h