| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
oran_tap_info Struct Reference

## Public Attributes
bool | userplane
uint16_t | eaxc
uint16_t | eaxc_du_port_id
uint16_t | eaxc_bandsector_id
uint16_t | eaxc_cc_id
uint16_t | eaxc_ru_port_id
bool | uplink
uint8_t | frame
uint8_t | slot
uint32_t | missing_sns
uint32_t | pdu_size
bool | section_types [SEC_C_MAX_INDEX]
uint16_t | section_ids [32+1]
uint8_t | num_section_ids
bool | extensions [32+1]
uint32_t | num_prbs
uint32_t | num_res
bool | non_zero_re_in_current_prb
uint32_t | num_prbs_zero
uint32_t | num_res_zero
uint32_t | ul_delay_in_us
uint32_t | ul_delay_configured_max
uint32_t | compression_methods
uint32_t | compression_width
uint8_t | num_beams
uint16_t | beams [32]

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/epan/dissectors/packet-oran.h