| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
TAdsDeviceNotificationReq Struct Reference

Header structure for an ADS DeviceNotification request, preceding one or more AdsStampHeader entries. More...

`#include <packet-ams.h>`

## Public Attributes
uint32_t | cbLength
uint32_t | nStamps

## Detailed Description

Header structure for an ADS DeviceNotification request, preceding one or more AdsStampHeader entries.

## Member Data Documentation

## ◆ cbLength

uint32_t TAdsDeviceNotificationReq::cbLength

Total length in bytes of the notification data payload that follows this header.

## ◆ nStamps

uint32_t TAdsDeviceNotificationReq::nStamps

Number of AdsStampHeader entries contained within the notification data payload.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/plugins/epan/ethercat/packet-ams.h