| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
_io_graph_settings_t Struct Reference

Persisted configuration for a single I/O Graph plot, corresponding to one UAT row. More...

`#include <io_graph_dialog.h>`

## Public Attributes
bool | enabled
bool | asAOT
char * | name
char * | dfilter
unsigned | color
uint32_t | style
uint32_t | yaxis
char * | yfield
uint32_t | sma_period
double | y_axis_factor

## Detailed Description

Persisted configuration for a single I/O Graph plot, corresponding to one UAT row.

## Member Data Documentation

## ◆ asAOT

bool _io_graph_settings_t::asAOT

True if this graph should be drawn always-on-top of others

## ◆ color

unsigned _io_graph_settings_t::color

Plot colour encoded as a packed RGB value

## ◆ dfilter

char* _io_graph_settings_t::dfilter

Display filter string restricting which packets contribute to this graph

## ◆ enabled

bool _io_graph_settings_t::enabled

True if this graph is active and should be rendered

## ◆ name

char* _io_graph_settings_t::name

User-visible display name for this graph

## ◆ sma_period

uint32_t _io_graph_settings_t::sma_period

Simple Moving Average period in number of intervals; 0 disables SMA

## ◆ style

uint32_t _io_graph_settings_t::style

Plot style (e.g. line, impulse, bar, dot); maps to a ::io_graph_plot_style value

## ◆ y_axis_factor

double _io_graph_settings_t::y_axis_factor

Multiplicative scaling factor applied to all Y-axis values before plotting

## ◆ yaxis

uint32_t _io_graph_settings_t::yaxis

Y-axis unit or aggregate mode (see io_graph_item_unit_t)

## ◆ yfield

char* _io_graph_settings_t::yfield

Display filter field whose value is used for Y-axis calculations

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/ui/qt/io_graph_dialog.h