| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
TAdsAddDeviceNotificationReq Struct Reference

Request structure for the ADS AddDeviceNotification command. More...

`#include <packet-ams.h>`

## Public Attributes
uint32_t | indexGroup
uint32_t | indexOffset
AdsNotificationAttrib | noteAttrib

## Detailed Description

Request structure for the ADS AddDeviceNotification command.

## Member Data Documentation

## ◆ indexGroup

uint32_t TAdsAddDeviceNotificationReq::indexGroup

Index group of the data item on the target device to monitor.

## ◆ indexOffset

uint32_t TAdsAddDeviceNotificationReq::indexOffset

Index offset within the index group of the data item to monitor.

## ◆ noteAttrib

AdsNotificationAttrib TAdsAddDeviceNotificationReq::noteAttrib

Notification attributes controlling delivery mode, timing, and comparison limits.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/plugins/epan/ethercat/packet-ams.h