| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
_tap_imsi_info_t Struct Reference

`#include <packet-e212.h>`

## Public Attributes
uint32_t | frame_number
const char * | imsi
address | src_addr
address | dst_addr
const char * | protocol

## Detailed Description

Structure passed via the "imsi" tap for each associated IMSI event.

## Member Data Documentation

## ◆ dst_addr

address _tap_imsi_info_t::dst_addr

Destination address of the packet

## ◆ frame_number

uint32_t _tap_imsi_info_t::frame_number

Frame number where IMSI was associated

## ◆ imsi

const char* _tap_imsi_info_t::imsi

IMSI string

## ◆ protocol

const char* _tap_imsi_info_t::protocol

Protocol name (e.g. "GTPv2", "PFCP")

## ◆ src_addr

address _tap_imsi_info_t::src_addr

Source address of the packet

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/epan/dissectors/packet-e212.h