| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
blf_ethernet_phystate Struct Reference

Header for a BLF Ethernet PHY state event object reporting a physical layer state transition. More...

`#include <blf.h>`

## Public Attributes
uint16_t | channel
uint16_t | flags
uint8_t | phyState
uint8_t | phyEvent
uint8_t | hardwareChannel
uint8_t | res1

## Detailed Description

Header for a BLF Ethernet PHY state event object reporting a physical layer state transition.

## Member Data Documentation

## ◆ channel

uint16_t blf_ethernet_phystate::channel

Logical Ethernet channel number to which this PHY state event applies.

## ◆ flags

uint16_t blf_ethernet_phystate::flags

Bitmask of flags indicating which optional fields in this record are valid.

## ◆ hardwareChannel

uint8_t blf_ethernet_phystate::hardwareChannel

Hardware channel index corresponding to this logical channel.

## ◆ phyEvent

uint8_t blf_ethernet_phystate::phyEvent

PHY event that triggered this state change (e.g. link up, link down, error).

## ◆ phyState

uint8_t blf_ethernet_phystate::phyState

Current PHY state (e.g. idle, initializing, link ready).

## ◆ res1

uint8_t blf_ethernet_phystate::res1

Reserved; must be zero.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/wiretap/blf.h