| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
_DOT11DECRYPT_KEY_ITEM::DOT11DECRYPT_KEY_ITEMDATA_TK Struct Reference

Holds a Temporal Key (TK) and optional MLD MAC addresses for per-link decryption. More...

`#include <dot11decrypt_user.h>`

## Public Attributes
uint8_t | Tk [32]
uint8_t | Len
bool | mld
uint8_t | ap_mld_mac [6]
uint8_t | sta_mld_mac [6]

## Detailed Description

Holds a Temporal Key (TK) and optional MLD MAC addresses for per-link decryption.

## Member Data Documentation

## ◆ ap_mld_mac

uint8_t _DOT11DECRYPT_KEY_ITEM::DOT11DECRYPT_KEY_ITEMDATA_TK::ap_mld_mac[6]

Multi-Link Device MAC address of the AP; valid only when `mld` is true

## ◆ Len

uint8_t _DOT11DECRYPT_KEY_ITEM::DOT11DECRYPT_KEY_ITEMDATA_TK::Len

Length in bytes of the valid portion of `Tk`

## ◆ mld

bool _DOT11DECRYPT_KEY_ITEM::DOT11DECRYPT_KEY_ITEMDATA_TK::mld

True if this TK is associated with an MLO connection and the MLD MAC fields are valid

## ◆ sta_mld_mac

uint8_t _DOT11DECRYPT_KEY_ITEM::DOT11DECRYPT_KEY_ITEMDATA_TK::sta_mld_mac[6]

Multi-Link Device MAC address of the station; valid only when `mld` is true

## ◆ Tk

uint8_t _DOT11DECRYPT_KEY_ITEM::DOT11DECRYPT_KEY_ITEMDATA_TK::Tk[32]

Raw temporal key bytes used for unicast frame decryption

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/epan/crypt/dot11decrypt_user.h