| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
_ETYPE_88A4_NV_DATA_HEADER Struct Reference

Platform-independent header describing a single EtherType 0x88A4 non-volatile data entry; layout is fixed across all platforms. More...

`#include <packet-nv.h>`

## Public Attributes
uint16_t | Id
uint16_t | Hash
uint16_t | Length
uint16_t | Quality

## Detailed Description

Platform-independent header describing a single EtherType 0x88A4 non-volatile data entry; layout is fixed across all platforms.

## Member Data Documentation

## ◆ Hash

uint16_t _ETYPE_88A4_NV_DATA_HEADER::Hash

Hash of the NV data payload, used to detect corruption or unintended modification.

## ◆ Id

uint16_t _ETYPE_88A4_NV_DATA_HEADER::Id

Identifier of the NV data entry, used to distinguish the type or source of the payload.

## ◆ Length

uint16_t _ETYPE_88A4_NV_DATA_HEADER::Length

Length in bytes of the NV data payload that follows this header.

## ◆ Quality

uint16_t _ETYPE_88A4_NV_DATA_HEADER::Quality

Quality indicator for the NV data entry, reflecting validity or signal confidence.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/plugins/epan/ethercat/packet-nv.h