| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
ttl_entryheader Struct Reference

Per-entry header preceding each logged frame in a TTL capture file. More...

`#include <ttl.h>`

## Public Attributes
uint16_t | size_type
uint16_t | dest_addr
uint16_t | src_addr
uint16_t | status_info

## Detailed Description

Per-entry header preceding each logged frame in a TTL capture file.

## Member Data Documentation

## ◆ dest_addr

uint16_t ttl_entryheader::dest_addr

Packed field: meta flag bits in the upper 3 bits, destination address in the lower 13 bits.

## ◆ size_type

uint16_t ttl_entryheader::size_type

Packed field: entry type in the upper 4 bits, payload size in the lower 12 bits.

## ◆ src_addr

uint16_t ttl_entryheader::src_addr

Packed field: meta flag bits in the upper 3 bits, source address in the lower 13 bits.

## ◆ status_info

uint16_t ttl_entryheader::status_info

Status or auxiliary information whose meaning depends on the entry type in size_type.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/wiretap/ttl.h