| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
rlc_graph Struct Reference

Holds all state required to render an RLC sequence-number graph for one channel. More...

`#include <tap-rlc-graph.h>`

## Public Attributes
struct rlc_segment * | segments
struct rlc_segment * | last_segment
bool | channelSet
uint8_t | rat
uint16_t | ueid
uint16_t | channelType
uint16_t | channelId
uint8_t | rlcMode
uint8_t | direction

## Detailed Description

Holds all state required to render an RLC sequence-number graph for one channel.

## Member Data Documentation

## ◆ channelId

uint16_t rlc_graph::channelId

Logical channel ID of the graphed channel.

## ◆ channelSet

bool rlc_graph::channelSet

True if the channel identity fields below have been populated.

## ◆ channelType

uint16_t rlc_graph::channelType

Logical channel type of the graphed channel.

## ◆ direction

uint8_t rlc_graph::direction

Direction (uplink or downlink) of the graphed channel.

## ◆ last_segment

struct rlc_segment* rlc_graph::last_segment

Tail of the linked list, used for O(1) appends.

## ◆ rat

uint8_t rlc_graph::rat

Radio Access Technology of the graphed channel.

## ◆ rlcMode

uint8_t rlc_graph::rlcMode

RLC mode of the graphed channel.

## ◆ segments

struct rlc_segment* rlc_graph::segments

Head of the linked list of segments to be plotted.

## ◆ ueid

uint16_t rlc_graph::ueid

UE identifier of the graphed channel.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/ui/tap-rlc-graph.h