| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
erf_record Struct Reference

Endace Record Format (ERF) record header, common to all ERF record types. More...

`#include <erf_record.h>`

## Public Attributes
erf_timestamp_t | ts
uint8_t | type
uint8_t | flags
uint16_t | rlen
uint16_t | lctr
uint16_t | wlen

## Detailed Description

Endace Record Format (ERF) record header, common to all ERF record types.

## Member Data Documentation

## ◆ flags

uint8_t erf_record::flags

ERF flags: RX error, DS (duplicate/steer), truncation, and extension-header present bits.

## ◆ lctr

uint16_t erf_record::lctr

Loss counter or color/flow identifier, depending on record type.

## ◆ rlen

uint16_t erf_record::rlen

Record length in bytes, including this header, any extension headers, and payload.

## ◆ ts

erf_timestamp_t erf_record::ts

ERF timestamp; upper 32 bits = seconds, lower 32 bits = fractional.

## ◆ type

uint8_t erf_record::type

ERF record type (e.g. `TYPE_ETH`, `TYPE_HDLC_POS`, `TYPE_AAL5`).

## ◆ wlen

uint16_t erf_record::wlen

Wire length: original packet size on the medium before any truncation.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/wiretap/erf_record.h