| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
blf_linmessagedescriptor Struct Reference

BLF LIN message descriptor, extending the sync field event with frame identification and protocol metadata. More...

`#include <blf.h>`

## Public Attributes
blf_linsynchfieldevent_t | linSynchFieldEvent
uint16_t | supplierId
uint16_t | messageId
uint8_t | configuredNodeAddress
uint8_t | id
uint8_t | dlc
uint8_t | checksumModel

## Detailed Description

BLF LIN message descriptor, extending the sync field event with frame identification and protocol metadata.

## Member Data Documentation

## ◆ checksumModel

uint8_t blf_linmessagedescriptor::checksumModel

Checksum model used: 0 = classic, 1 = enhanced.

## ◆ configuredNodeAddress

uint8_t blf_linmessagedescriptor::configuredNodeAddress

LIN 2.0+ configured node address (NAD) for the slave that owns this frame.

## ◆ dlc

uint8_t blf_linmessagedescriptor::dlc

Data Length Code indicating the number of data bytes (0–8).

## ◆ id

uint8_t blf_linmessagedescriptor::id

LIN frame identifier (0–63).

## ◆ linSynchFieldEvent

blf_linsynchfieldevent_t blf_linmessagedescriptor::linSynchFieldEvent

Sync field event carrying SOF, baud rate, and sync field timings.

## ◆ messageId

uint16_t blf_linmessagedescriptor::messageId

LIN 2.0: message identifier; LIN 2.1: position index as specified in the LDF.

## ◆ supplierId

uint16_t blf_linmessagedescriptor::supplierId

LIN 2.0+ supplier identifier associated with this frame's node.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/wiretap/blf.h