8.27. UDP Multicast Streams
Prev | Chapter 8. Statistics | Next

## 8.27. UDP Multicast Streams

The UDP Multicast Streams window shows statistics for all UDP multicast streams. It includes source addresses and ports, destination addresses and ports, packets counter and other data. You can specify the burst interval, the alarm limits and output speeds. To apply new settings, press Enter.

With these statistics you can:

- Measure the burst size for a video stream. The `Burst measurement interval` and `Burst alarm threshold` settings are used by the sliding window algorithm to compute how many times the threshold was hit, and is shown in `Burst Alarms`. The threshold may be hit several times during a same window.
- Measure the output buffer size limit such that no packet drop will occur. The `Stream empty speed` and `Buffer alarm threshold` settings are used by the Leaky bucket algorithm to compute how many times the buffer was filled while a client was at the same time emptying it at a given, constant speed. When filled, the maximum seen is stored in `Max Buffer` and `Buffer Alarms` is incremented (note that it won’t be incremented again until the buffer value first goes below the threshold, hence a high value of alarms when the chosen threshold is near the minimum necessary one). The `Total empty speed` plays the same role when considering all the flows added.
- Detect the packet loss inside the MPEG2 video stream.

| Note
While this dialog helps diagnosing bursts of traffic, or inappropriate small buffers, it doesn’t bring information on traffic drops or buffer starvations. You can use the Section 8.8, “The “I/O Graphs” Window” to seek such behaviors.

Figure 8.16. UDP Multicast Streams window

Prev | Up | Next
8.26. TCP Stream Graphs | Home | 8.28. Reliable Server Pooling (RSerPool)