8.21. HART-IP
Prev | Chapter 8. Statistics | Next

## 8.21. HART-IP

Highway Addressable Remote Transducer over IP (HART-IP) is an application layer protocol. It sends and receives digital information between smart devices and control or monitoring systems. The HART-IP statistics window shows the counter for response, request, publish and error packets. You can filter, copy or save the data to a file.

Prev | Up | Next
8.20. Flow Graph | Home | 8.22. HPFEEDS