| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
i4b_trace_setupa_t Struct Reference

Configuration parameters specifying which ISDN controller units and channels to trace. More...

`#include <i4b_trace.h>`

## Public Attributes
int32_t | rxunit
int32_t | rxflags
int32_t | txunit
int32_t | txflags

## Detailed Description

Configuration parameters specifying which ISDN controller units and channels to trace.

## Member Data Documentation

## ◆ rxflags

int32_t i4b_trace_setupa_t::rxflags

Bitmask selecting the RX channel(s) to trace (D channel and/or B channel).

## ◆ rxunit

int32_t i4b_trace_setupa_t::rxunit

Controller unit number from which to capture received (RX) frames.

## ◆ txflags

int32_t i4b_trace_setupa_t::txflags

Bitmask selecting the TX channel(s) to trace (D channel and/or B channel).

## ◆ txunit

int32_t i4b_trace_setupa_t::txunit

Controller unit number from which to capture transmitted (TX) frames.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/wiretap/i4b_trace.h