| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
blf_lincrcerror2 Struct Reference

Header for a BLF LIN CRC error event object (version 2). More...

`#include <blf.h>`

## Public Attributes
blf_lindatabytetimestampevent_t | linDataByteTimestampEvent
uint8_t | data [8]
uint16_t | crc
uint8_t | dir
uint8_t | fsmId
uint8_t | fsmState
uint8_t | simulated
uint8_t | res1 [2]

## Detailed Description

Header for a BLF LIN CRC error event object (version 2).

## Member Data Documentation

## ◆ crc

uint16_t blf_lincrcerror2::crc

Erroneous checksum value received on the bus.

## ◆ data

uint8_t blf_lincrcerror2::data[8]

Payload data bytes received before the CRC error was detected.

## ◆ dir

uint8_t blf_lincrcerror2::dir

Transfer direction: 0 = RX, 1 = TX Receipt, 2 = TX Request.

## ◆ fsmId

uint8_t blf_lincrcerror2::fsmId

Finite state machine instance identifier (obsolete).

## ◆ fsmState

uint8_t blf_lincrcerror2::fsmState

Finite state machine state at time of capture (obsolete).

## ◆ linDataByteTimestampEvent

blf_lindatabytetimestampevent_t blf_lincrcerror2::linDataByteTimestampEvent

Data byte timestamp event carrying sync, descriptor, and per-byte timestamps.

## ◆ res1

uint8_t blf_lincrcerror2::res1[2]

Reserved; must be zero.

## ◆ simulated

uint8_t blf_lincrcerror2::simulated

Frame origin: 0 = real frame captured on bus, 1 = simulated frame.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/wiretap/blf.h