| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
blf_linbusevent Struct Reference

Base event header for BLF LIN bus events, carrying start-of-frame timing and baud rate. More...

`#include <blf.h>`

## Public Attributes
uint64_t | sof
uint32_t | eventBaudrate
uint16_t | channel
uint8_t | res1 [2]

## Detailed Description

Base event header for BLF LIN bus events, carrying start-of-frame timing and baud rate.

## Member Data Documentation

## ◆ channel

uint16_t blf_linbusevent::channel

Logical LIN channel number on which this event was observed.

## ◆ eventBaudrate

uint32_t blf_linbusevent::eventBaudrate

Baud rate in bits per second measured for this LIN bus event.

## ◆ res1

uint8_t blf_linbusevent::res1[2]

Reserved; must be zero.

## ◆ sof

uint64_t blf_linbusevent::sof

Start-of-frame timestamp in nanoseconds relative to the measurement start.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/wiretap/blf.h