| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
_sctp_addr_chunk Struct Reference

Tracks per-address chunk counts for one direction of an SCTP association. More...

`#include <tap-sctp-analysis.h>`

## Public Attributes
uint32_t | direction
address | addr
uint32_t | addr_count [256]

## Detailed Description

Tracks per-address chunk counts for one direction of an SCTP association.

## Member Data Documentation

## ◆ addr

address _sctp_addr_chunk::addr

The peer address this record tracks.

## ◆ addr_count

uint32_t _sctp_addr_chunk::addr_count[256]

Per-chunk-type packet count for this address, indexed by SCTP chunk type.

## ◆ direction

uint32_t _sctp_addr_chunk::direction

Direction this record applies to (endpoint 1 or 2).

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/ui/tap-sctp-analysis.h