| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Functions
busmaster.h File Reference
`#include <wiretap/wtap.h>`

Go to the source code of this file.

## Functions
wtap_open_return_val | busmaster_open (wtap *wth, int *err, char **err_info)
| Opens a file using the Busmaster log reader.

## Detailed Description

Wiretap Library Copyright (c) 1998 by Gilbert Ramirez gram@.nosp@m.alum.nosp@m.ni.ri.nosp@m.ce.e.nosp@m.du

Support for Busmaster log file format Copyright (c) 2019 by Maksim Salau maksi.nosp@m.m.sa.nosp@m.lau@g.nosp@m.mail.nosp@m..com

SPDX-License-Identifier: GPL-2.0-or-later

## Function Documentation

## ◆ busmaster_open()

wtap_open_return_val busmaster_open | ( | wtap * | wth,
|  | int * | err,
|  | char ** | err_info )

Opens a file using the Busmaster log reader.

Parameters

  wth | Pointer to the wtap structure.
  err | Pointer to an integer that will hold any error code.
  err_info | Pointer to a string that will hold any error information.

Returns
  int WTAP_OPEN_OK if successful, otherwise an error code.

< Precision: 1 microsecond (6 fractional digits).