| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
ws80211_interface Struct Reference

Represents a wireless network interface and its capture capabilities. More...

`#include <ws80211_utils.h>`

## Public Attributes
char * | ifname
bool | can_set_freq
bool | can_check_fcs
GArray * | bands
int | cap_monitor

## Detailed Description

Represents a wireless network interface and its capture capabilities.

## Member Data Documentation

## ◆ bands

GArray* ws80211_interface::bands

Array of ws80211_band structs indexed by ws80211_band_type; always non-NULL but may contain fewer entries than the total number of defined band types

## ◆ can_check_fcs

bool ws80211_interface::can_check_fcs

True if the interface supports FCS validation filtering

## ◆ can_set_freq

bool ws80211_interface::can_set_freq

True if the interface supports setting the operating frequency

## ◆ cap_monitor

int ws80211_interface::cap_monitor

Non-zero if the interface supports monitor mode capture

## ◆ ifname

char* ws80211_interface::ifname

Interface name (e.g., "wlan0")

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/capture/ws80211_utils.h