| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
ws_manuf_iter Struct Reference

Internal iterator state for traversing all manufacturer entries across the 24-, 28-, and 36-bit OUI tables. More...

`#include <manuf.h>`

## Public Attributes
size_t | idx24
size_t | idx28
size_t | idx36
struct ws_manuf | buf24
struct ws_manuf | buf28
struct ws_manuf | buf36

## Detailed Description

Internal iterator state for traversing all manufacturer entries across the 24-, 28-, and 36-bit OUI tables.

Not intended for direct access by users; use the provided iterator API instead.

## Member Data Documentation

## ◆ buf24

struct ws_manuf ws_manuf_iter::buf24

Buffered current entry from the 24-bit OUI table.

## ◆ buf28

struct ws_manuf ws_manuf_iter::buf28

Buffered current entry from the 28-bit OUI table.

## ◆ buf36

struct ws_manuf ws_manuf_iter::buf36

Buffered current entry from the 36-bit OUI table.

## ◆ idx24

size_t ws_manuf_iter::idx24

Current position within the 24-bit (MA-L) OUI table.

## ◆ idx28

size_t ws_manuf_iter::idx28

Current position within the 28-bit (MA-M) OUI table.

## ◆ idx36

size_t ws_manuf_iter::idx36

Current position within the 36-bit (MA-S) OUI table.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/epan/manuf.h