| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
ieee_802_11g Struct Reference

PHY metadata for 802.11g OFDM captures. More...

`#include <wtap.h>`

## Public Attributes
unsigned | has_mode: 1
uint32_t | mode

## Detailed Description

PHY metadata for 802.11g OFDM captures.

This struct should only be used for packets transmitted using OFDM. Packets sent on an 802.11g network using DSSS should use ieee_802_11b with the PHY type set to 802.11b instead.

## Member Data Documentation

## ◆ has_mode

unsigned ieee_802_11g::has_mode

Non-zero if `mode` contains a valid value.

## ◆ mode

uint32_t ieee_802_11g::mode

Proprietary extension mode flags describing vendor-specific 802.11g transmission properties.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/wiretap/wtap.h