| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
_conversation_key_t Struct Reference

Composite hash table key identifying a conversation by its two endpoints and optional ID. More...

`#include <conversation_table.h>`

## Public Attributes
address | addr1
address | addr2
uint32_t | port1
uint32_t | port2
conv_id_t | conv_id

## Detailed Description

Composite hash table key identifying a conversation by its two endpoints and optional ID.

## Member Data Documentation

## ◆ addr1

address _conversation_key_t::addr1

Address of the first endpoint of the conversation

## ◆ addr2

address _conversation_key_t::addr2

Address of the second endpoint of the conversation

## ◆ conv_id

conv_id_t _conversation_key_t::conv_id

Optional conversation ID used to disambiguate conversations sharing the same address/port 4-tuple

## ◆ port1

uint32_t _conversation_key_t::port1

Transport port of the first endpoint

## ◆ port2

uint32_t _conversation_key_t::port2

Transport port of the second endpoint

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/epan/conversation_table.h