| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
gryphon_pkt_info_t Struct Reference

Tracks per-packet command state for matching Gryphon request and response frames within a dissection. More...

`#include <packet-gryphon.h>`

## Public Attributes
uint32_t | cmd
uint32_t | cmd_context
uint32_t | ioctl_command
uint32_t | req_frame_num
uint32_t | rsp_frame_num
nstime_t | req_time

## Detailed Description

Tracks per-packet command state for matching Gryphon request and response frames within a dissection.

## Member Data Documentation

## ◆ cmd

uint32_t gryphon_pkt_info_t::cmd

Gryphon command code identifying the type of operation for this packet.

## ◆ cmd_context

uint32_t gryphon_pkt_info_t::cmd_context

Context value associated with the command; stored as uint32_t to allow future expansion beyond a single byte.

## ◆ ioctl_command

uint32_t gryphon_pkt_info_t::ioctl_command

IOCTL command code; currently the sole user of this field, intended to be generalised in future.

## ◆ req_frame_num

uint32_t gryphon_pkt_info_t::req_frame_num

Wireshark frame number of the request packet associated with this transaction.

## ◆ req_time

nstime_t gryphon_pkt_info_t::req_time

Timestamp of the request packet, used to calculate request/response latency.

## ◆ rsp_frame_num

uint32_t gryphon_pkt_info_t::rsp_frame_num

Wireshark frame number of the response packet associated with this transaction.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/plugins/epan/gryphon/packet-gryphon.h