| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
_tap_rtp_save_data_t Struct Reference

Holds the minimal per-packet data needed when saving an RTP stream's payload to file. More...

`#include <tap-rtp-analysis.h>`

## Public Attributes
uint32_t | timestamp
unsigned int | payload_type
size_t | payload_len

## Detailed Description

Holds the minimal per-packet data needed when saving an RTP stream's payload to file.

## Member Data Documentation

## ◆ payload_len

size_t _tap_rtp_save_data_t::payload_len

Length in bytes of the RTP payload to be saved.

## ◆ payload_type

unsigned int _tap_rtp_save_data_t::payload_type

RTP payload type identifying the codec or format of the payload.

## ◆ timestamp

uint32_t _tap_rtp_save_data_t::timestamp

RTP timestamp of the packet, used for reordering and timing during save.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/ui/tap-rtp-analysis.h