| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
blf_wlanframeheader Struct Reference

Header for a BLF WLAN frame object. More...

`#include <blf.h>`

## Public Attributes
uint16_t | channel
uint16_t | flags
uint8_t | direction
uint8_t | radio_channel
uint16_t | signal_strength
uint16_t | signal_quality
uint16_t | frame_length
uint32_t | res

## Detailed Description

Header for a BLF WLAN frame object.

## Member Data Documentation

## ◆ channel

uint16_t blf_wlanframeheader::channel

Logical channel number on which this frame was captured.

## ◆ direction

uint8_t blf_wlanframeheader::direction

Transfer direction: one of BLF_DIR_RX, BLF_DIR_TX, or BLF_DIR_TX_RQ.

## ◆ flags

uint16_t blf_wlanframeheader::flags

WLAN-specific flags for this frame.

## ◆ frame_length

uint16_t blf_wlanframeheader::frame_length

Total length in bytes of the captured WLAN frame.

## ◆ radio_channel

uint8_t blf_wlanframeheader::radio_channel

RF channel number on which this frame was transmitted or received.

## ◆ res

uint32_t blf_wlanframeheader::res

Reserved; must be zero.

## ◆ signal_quality

uint16_t blf_wlanframeheader::signal_quality

Received signal quality indicator.

## ◆ signal_strength

uint16_t blf_wlanframeheader::signal_strength

Received signal strength in dBm.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/wiretap/blf.h