| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
nr_sack_chunk_header Struct Reference

SCTP NR-SACK chunk header structure. More...

`#include <sctp_graph_dialog.h>`

## Public Attributes
uint8_t | type
uint8_t | flags
uint16_t | length
uint32_t | cum_tsn_ack
uint32_t | a_rwnd
uint16_t | nr_of_gaps
uint16_t | nr_of_nr_gaps
uint16_t | nr_of_dups
uint16_t | reserved
struct gaps | gaps [1]

## Detailed Description

SCTP NR-SACK chunk header structure.

## Member Data Documentation

## ◆ a_rwnd

uint32_t nr_sack_chunk_header::a_rwnd

Advertised Receiver Window Credit (a_rwnd).

## ◆ cum_tsn_ack

uint32_t nr_sack_chunk_header::cum_tsn_ack

Cumulative TSN Ack.

## ◆ flags

uint8_t nr_sack_chunk_header::flags

Chunk flags.

## ◆ gaps

struct gaps nr_sack_chunk_header::gaps[1]

A Flexible Array Member (standard C, not standard C++)

## ◆ length

uint16_t nr_sack_chunk_header::length

Length of the chunk.

## ◆ nr_of_dups

uint16_t nr_sack_chunk_header::nr_of_dups

Number of duplicate TSNs.

## ◆ nr_of_gaps

uint16_t nr_sack_chunk_header::nr_of_gaps

Number of gap blocks.

## ◆ nr_of_nr_gaps

uint16_t nr_sack_chunk_header::nr_of_nr_gaps

Number of Non-Renegable gap blocks.

## ◆ reserved

uint16_t nr_sack_chunk_header::reserved

Reserved field.

## ◆ type

uint8_t nr_sack_chunk_header::type

Type of the chunk.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/ui/qt/sctp_graph_dialog.h