| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
isdn_phdr Struct Reference

Pseudo-header for ISDN capture files carrying direction and channel metadata. More...

`#include <wtap.h>`

## Public Attributes
bool | uton
uint8_t | channel

## Detailed Description

Pseudo-header for ISDN capture files carrying direction and channel metadata.

## Member Data Documentation

## ◆ channel

uint8_t isdn_phdr::channel

Logical channel number: 0 = D-channel (signalling), n = B-channel n (bearer).

## ◆ uton

bool isdn_phdr::uton

Direction of the packet: true = user-to-network (UNI), false = network-to-user.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/wiretap/wtap.h