| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
blf_linsenderror Struct Reference

Header for a BLF LIN send error event object (legacy format). More...

`#include <blf.h>`

## Public Attributes
uint16_t | channel
uint8_t | id
uint8_t | dlc
uint8_t | fsmId
uint8_t | fsmState
uint8_t | headerTime
uint8_t | fullTime

## Detailed Description

Header for a BLF LIN send error event object (legacy format).

## Member Data Documentation

## ◆ channel

uint16_t blf_linsenderror::channel

Logical LIN channel number on which the send error was observed.

## ◆ dlc

uint8_t blf_linsenderror::dlc

Data Length Code of the frame that failed to send.

## ◆ fsmId

uint8_t blf_linsenderror::fsmId

Identifier of the finite state machine instance that processed this frame.

## ◆ fsmState

uint8_t blf_linsenderror::fsmState

State of the finite state machine at the time the send error occurred.

## ◆ fullTime

uint8_t blf_linsenderror::fullTime

Total duration of the LIN frame up to the error in bit times.

## ◆ headerTime

uint8_t blf_linsenderror::headerTime

Duration of the LIN header in bit times.

## ◆ id

uint8_t blf_linsenderror::id

LIN frame identifier (0–63) of the frame that failed to send.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/wiretap/blf.h