| Wireshark 4.7.3 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
_EtherCATFrameParser Union Reference

EtherCAT frame header, giving access to the 16-bit header word both as individual bit-fields and as a raw value. More...

`#include <packet-ethercat-frame.h>`

## Public Attributes
struct { |
uint16_t length: 11 |
uint16_t reserved: 1 |
uint16_t protocol: 4 |
} | v
uint16_t | hdr

## Detailed Description

EtherCAT frame header, giving access to the 16-bit header word both as individual bit-fields and as a raw value.

## Member Data Documentation

## ◆ hdr

uint16_t _EtherCATFrameParser::hdr

Raw 16-bit header word.

## ◆ length

uint16_t _EtherCATFrameParser::length

Total byte length of all datagrams in the frame.

## ◆ protocol

uint16_t _EtherCATFrameParser::protocol

Protocol type identifier (0x1 = EtherCAT commands).

## ◆ reserved

uint16_t _EtherCATFrameParser::reserved

Reserved; must be zero.

## ◆ [struct]

struct { ... } _EtherCATFrameParser::v

Structured bit-field access to the header.

The documentation for this union was generated from the following file:

- /builds/wireshark/wireshark/plugins/epan/ethercat/packet-ethercat-frame.h